

Hanwha Techwin is a leading supplier of advanced video surveillance solutions for IP-video, analog and hybrid systems. Building on the company's history of innovation, Hanwha Techwin is dedicated to providing systems solutions with the highest levels of performance, reliability and cost-efficiency. Hanwha Techwin is committed to the continued development of innovative systems products for professional security applications.

For additional information, visit http://www.hanwha-security.com/

**VGA NETWORK THERMAL CAMERA**

**DIVISION 28 – ELECTRONIC SAFETY AND SECURITY**

**Notes to Specifier:**

1. Where several alternative parameters or specifications exist, or where, the specifier has the option of inserting text, such choices are presented in **<bold text>.**

2. Explanatory notes and comments are presented in **colored** text.

**Important: See further notes on the following page.**

**Important Note to Security Systems Specifiers**

CSI MasterFormat 2016 incorporates numerous significant changes affecting electronic safety and security. This document is written to provide flexibility in using either format, although adoption of MasterFormat 2016 is encouraged. The following is a guide to the MasterFormat numbers relevant to the product referenced in this specification.

**Primary Specification Area:**

MasterFormat 2014:

28 20 00 Electronic Surveillance

28 23 00 Video Surveillance

28 23 29 Video Surveillance Remote Devices and Sensors

MasterFormat 2016:

28 20 00 Video Surveillance

28 2x xx Surveillance Cameras

28 2x xx IP Cameras

**Related Requirements:**

MasterFormat 2014:

27 20 00 Data Communications

28 23 13 Video Surveillance Control and Management Systems

28 23 16 Video Surveillance Monitoring and Supervisory Interfaces

28 23 19 Digital Video Recorders and Analog Recording Devices

28 23 23 Video Surveillance Systems Infrastructure

MasterFormat 2016

27 15 01.xx Video Surveillance Communications Conductors and Cables

27 20 00 Data Communications

28 05 xx.xx PoE Power Sources for Electronic Safety and Security

28 05 xx Storage Appliances for Electronic Safety and Security

28 05 xx.xx Network Video Recorders

28 05 xx Cyber Requirements for Electronic Safety and Security

28 05 xx Safety and Security Network Communications Equipment

28 2x 00 Video Management System

**VGA NETWORK THERMAL CAMERA**

1. **GENERAL**
   1. **SUMMARY**
      1. Section includes a VGA Thermal IP camera with explosion-proof certificates.
      2. Product – VGA Thermal camera, with multi-streaming (H.264 and MJPEG) capability.

## Related Requirements

**Refer to MasterFormat notes at the beginning of this document to select requirements specific to the MasterFormat version being used in the specification.**

* 1. **REFERENCES**
     1. Abbreviations
        1. AGC Auto Gain Control
        2. AES Advanced Encryption Standard
        3. API Application Programming Interface
        4. ARP Address Resolution Protocol
        5. AWB Auto White Balance
        6. BLC Back light compensation
        7. CBR Constant Bit Rate
        8. CVBS Composite Video Blanking and Sync
        9. DHCP Dynamic Host Configuration Protocol
        10. DNR Digital Noise Reduction
        11. DNS Domain Name Server
        12. DDNS Dynamic Domain Name Server
        13. DSCP Differentiated Services Code Point
        14. fps frames per second
        15. FTP File Transfer Protocol
        16. GOV Group of Video
        17. GUI Graphical User Interface
        18. HD High Definition
        19. HTTP Hypertext Transfer Protocol
        20. HTTPS Secure HTTP
        21. ICMP Internet Control Message Protocol
        22. IGMP Internet Group Management Protocol
        23. IP Internet Protocol
        24. IR Infrared
        25. JPEG Joint Photographic Experts Group
        26. LAN Local Area Network
        27. LED Light Emitting Diode
        28. LDC Lens Distortion Correction
        29. LLDP Link Layer Discovery Protocol
        30. LPR License Plate Recognition
        31. MJPEG Motion JPEG
        32. MP Megapixel
        33. MPEG Moving Pictures Experts Group
        34. NAS Network Attached Storage
        35. NTP Network Time Protocol
        36. NVR Network Video Recorder
        37. PIM-SM Protocol Independent Multicast-Sparse Mode
        38. PoE Power over Ethernet
        39. PPPoE Point to Point Protocol over Ethernet
        40. QoS Quality of Service
        41. RTP Real-Time Transport Protocol
        42. RTCP Real-Time Control Protocol
        43. RTSP Real-Time Streaming Protocol
        44. SDK Software Development Kit
        45. SFP Small Form factor Pluggable
        46. SMTP Simple Mail Transfer Protocol
        47. SNMP Simple Network Management Protocol
        48. SSDR Super Smart Dynamic Range
        49. SSNR Super Smart Noise Reduction
        50. SSL Secure Sockets Layer
        51. TCP Transmission Control Protocol
        52. UDP User Datagram Protocol
        53. UPnP Universal Plug and Play
        54. VBR Variable Bit Rate
        55. VMS Video Management System
        56. WDR Wide Dynamic Range
        57. LCE Local Contrast Enhancement
     2. Reference Standards
        1. Network - IEEE
           1. 802.3 Ethernet Standards
           2. 802.1x Port-based Network Access Control
           3. IPv4 IP addressing version 4
           4. IPv6 IP addressing version 6
           5. QoS Quality of Service
        2. Video
           1. ISO / IEC 23008-2:2013, MPEG-H Part2 (ITU H.265, HEVC)
           2. ISO / IEC 14496–10, MPEG-4 Part 10 ( ITU H.264)
           3. ISO / IEC 10918 – JPEG
           4. ONVIF – Profiles S / G
        3. EMC & Safety
           1. FCC-47 CFR Part 15 Subpart B Class B

ANSI C63.4-2014 Class A

* + - * 1. IC Regulation ICES-003 : 2016

ANSI C63.4-2014 Class A

* + - * 1. CE EMC-Directive 2014/30/EU

EN 55032:2015 Class A

EN 50130-4:2011+A1:2014

EN 61000-3-2:2014

EN 61000-3-3:2013

* + - * 1. VCCI-CISPR 32: Class A
        2. VCCI-CISPR 32: Class A
        3. AS/NZS CISPR32:2015 Class A
        4. UL listed
        5. CE EN 50581:2012 (hazardous substances)
      1. Ingress Protection and Vandal Resistance
         1. ANSI / IEC60529 – Degrees of protection Provided by Enclosures: IP66
         2. IEC EN 62262 - Degrees of protection provided by enclosures for electrical equipment against external mechanical impacts: IK10
         3. IEC 60068-2-75: IK10
         4. NEMA 4x - enclosures are made of stainless steel, aluminum, fiberglass, or polycarbonate. NEMA 4X enclosures are used in harsh environments where corrosive materials and caustic cleaners are used
    1. Definitions
       1. GOV (Group of Video object planes) - A set of video frames for H.264 and H.265 compression, indicating a collection of frames from the initial I-Frame (key frame) to the next I-Frame. GOV consists of 2 kinds of frames: I-Frame and P-Frame.
       2. Dynamic GOV – Dynamic assignment of GOV length based on the complexity of the scene to efficiently manage bitrate of the video stream and reduce the storage required.
       3. Multi-exposure wide dynamic range - Operation which automatically adjusts shutter speed to provide a wide range between dark and light areas visible at the same time, preventing backlighting issues. Long exposure is used for bright areas and a short exposure is used in dark areas.
       4. Dynamic fps – Dynamic assignment of fps (frames per seconds) based on the movement of object(s) in the scene to efficiently manage bitrate of the video stream and reduce the storage required.
       5. WiseStream – Technology that controls quantization parameter, fps, and GOV length in H.265 and H.264 to efficiently manage bitrate of the video stream and reduce the storage required.
  1. **SUBMITTALS**
     1. Product Data
        1. Manufacturer’s printed or electronic data sheets
        2. Manufacturer’s installation and operation manuals
        3. Warranty documentation
  2. **QUALIFICATIONS**
     1. Manufacturer shall have a minimum of five years’ experience in producing IP video equipment.
     2. Installers shall be trained and authorized by the Manufacturer to install, integrate, test, and commission the system.
  3. **DELIVERY, STORAGE AND HANDLING**
     1. Deliver the camera in the manufacturer’s original, unopened, undamaged container with identification labels intact.
     2. Store the camera in a temperature environment indicated in 2.04 Detailed Specification, protected from mechanical and environmental conditions as designated by the manufacturer.
  4. **WARRANTY, LICENSING AND SUPPORT**
     1. Manufacturer shall provide a limited 3 year warranty for the product to be free of defects in material and workmanship.
     2. Manufacturer shall provide embedded camera video analytics free of license charges.

END OF SECTION

1. **PRODUCTS**
   1. **EQUIPMENT**
      1. Manufacturer: Hanwha Techwin

http://www.hanwha-security.com/

* + 1. Model TNO-4041TR
    2. Alternates: None
  1. **GENERAL DESCRIPTION**
     1. Thermal VGA camera shall have a metal housing which can prevent any inside sparks caused by the electronic components from igniting gases and conductive dust and causing explosion in a hazardous area.
     2. Video Compression and Transmission – The camera shall have the following properties relating to the video signals it produces.
        1. H.265, H.264 and MJPEG compression, each derived from a dedicated encoder and capable of being streamed independently and simultaneously
           1. H.265, H.264 – maximum of 30 fps at all resolution
           2. MJPEG – maximum of 30 fps at all resolution
        2. The camera shall be able to configure up to 10 independent video stream profiles with differing encoding, quality, frame rate, resolution, and bit rate settings.
        3. The camera shall be able to configure various resolution selections
           1. 16:9 aspect ratio : 640 x 360
           2. 4:3 aspect ratio : 640 x 480, 320 x 240
        4. The camera shall support unicast video streaming up to 20 users.
        5. The camera shall support multicast video streaming
        6. The camera shall be able to configure Dynamic DNS (DDNS). DDNS shall be provided with no additional cost by the manufacturer.
        7. The camera shall provide WiseStream Ⅱ, Dynamic GOV and Dynamic fps to efficiently manage bit rate of the video stream and reduce storage.
     3. Camera – The camera device shall have the following physical and performance properties:
        1. IK10 rated for protection against impacts.
        2. Dust proof and water proof (IP66 rated)
        3. NEMA 4X
        4. The camera shall be able to configure 32 privacy masking areas with polygons.
     4. Intelligence and Analytics – The camera shall have a suite of intelligent analytic functions.
        1. Motion detection with 8 definable detection areas with 8 point polygonal zones, and minimum/maximum object size.
        2. Detection of logical events of specified conditions from the camera’s video input
           1. Tampering, Loitering, Directional Detection, Virtual Line, Enter/Exit, Appear/Disappear
           2. Motion Detection, Audio Detection, Sound Classification
           3. Shock Detection
           4. Temperature Detection
     5. Interoperability – The camera shall be ONVIF Profile S and G compliant.
     6. The camera shall possess the following further characteristics:
        1. Built-in web server, accessed via non-plugin browsers including Google Chrome, IE11, MS Edge, Mozilla Firefox and Apple Safari.
        2. Micro SD/SDHC/SDXC memory card with configurable pre-alarm and post-alarm recording intervals
        3. NAS recording option with configurable pre-alarm and post-alarm recording intervals
        4. Alarms and notifications
           1. Alarm notification triggers:

Alarm input

Motion detection

Video & Audio analytics

Network disconnect

* + - * 1. Available notification means upon trigger:

File upload via FTP and e-mail

Notification via e-mail

Local storage (SD / SDHC / SDXC) or NAS recording at event triggers

External output

* + - 1. Pixel Counter available in the web viewer
      2. PoE capable
      3. IP66, IK10, NEMA 4x capable
      4. PT driver type
  1. **CAMERA SOFTWARE**
     1. The camera shall have a built in web server which supports non-plugin browsers including Google Chrome, IE11, MS Edge, Mozilla Firefox and Apple Safari from a PC or Mac.
     2. The web viewer shall provide a monitoring screen which displays live camera video and simultaneously provides same-screen access to the following functions:
        1. Live view window size
        2. Resolution setting
        3. Image (snapshot) capture
        4. Manual recording to SD or NAS
        5. Audio and Microphone control
        6. Access recorded data playback and camera configuration menus
        7. Alarm out are supported with two ports
        8. Temperature display on live view in real time
     3. The web viewer shall provide a playback screen which provides access to the following functions:
        1. Recorded data search using date and time range
        2. Recorded data search using event type
        3. Play a recorded video by event triggering
        4. Set resolution
        5. Play audio if present
        6. Generate a backup copy of saved video data
     4. The web viewer shall provide a setup screen which provides access to the following configuration settings and functions in the camera:
        1. Digital video profile to include compression type, maximum or target bit rate, frame rate, multicast parameters, crop encoding area
        2. User profile to include password, access level, authentication
        3. Date and time
        4. Network settings and IP version
           1. DDNS
           2. SSL, including certificate management
           3. IP Filtering
           4. 802.1x authentication
           5. Quality of Service settings
           6. SNMP to include version selection and settings
           7. Auto configuration
        5. Video setup
           1. Flip / mirror mode
           2. Hallway view
           3. Video output type
           4. Privacy zone
        6. Audio setup to include source, audio codec type, gain and bit rate.
        7. Camera settings to configure image preset, SSDR, LCE, exposure, DIS, sharpness, contrast, color level and on-screen display.
        8. Temperature setup to configure temperature unit, color patterns, spot emissivity and color bar.
        9. Event detection setup to configure notification parameters, recording rules, time schedule, tamper protection, motion detection, temperature detection and event triggers.
        10. Analytics setup to configure temperature detection, shock detection, motion detection, tampering detection, IVA, audio detection and sound classification.
        11. System function to control reboot, upgrade, check system and event logs and application (SDK) management.
        12. View profile information
     5. Client requirements
        1. Acceptable Operating Systems: Windows 7 / 8.1 / 10, MAC OS X 10.10, 10.11, 10.12
        2. Acceptable browsers:
           1. Non-plugin WebViewer Google Chrome, IE11, MS Edge, Mozilla Firefox,

Safari (Mac OS X only)

* 1. **DETAILED SPECIFICATIONS**
     1. Video
        1. Imaging device Uncooled Microbolometer
        2. Image Pixels 17um
        3. Effective Pixels 640(H) x 480(V)
        4. NETD < 50mK
        5. Video Out CVBS : 1.0 Vp-p / 75Ω composite, 720 x 480(N), 720 x 576(P),   
            for installation
     2. Lens
        1. Focal length 19mm Fixed
        2. Max. Aperture Ratio F1.0
        3. Field of View H: 32˚, V: 24.3°, D: 39.2°
        4. Min. Object Distance 11m (36.09ft)
        5. Focus Control Fixed
        6. Mount Type Board-in Type
     3. Radiometry
        1. Temperature detect range -20°C ~ 130°C(-4°F ~ 266°F)
        2. Temperature accuracy ±5°C (≤100°C ), ±20°C(＞100°C )
        3. Temperature detection Off / On(3ea Rectangle)
        4. Additional Hybrid palettes, Spot temperature reading
     4. Operational Functions
        1. Camera Title Off / On (Displayed up to 85 characters)
           1. W/W English / Numeric / Special characters
           2. China English / Chinese / Numeric / Special characters
           3. Common Multi-line (Max. 5), Color (Grey/Green/Red/Blue/Black/White),

Transparency, Auto scale by resolution

* + - 1. Motion Detection Off / On (8ea, 8-point polygonal)
      2. Privacy Masking Off / On (32 zones, polygonal)

- Color: Gray / Green / Red / Blue / Black / White

- Mosaic

* + - 1. Image Rotation Flip: Off / On

Mirror: Off / On

Hallway view: 0˚ / 90˚ / 270˚

* + - 1. Digital Image Stabilization Off / On (Built-in Gyro Sensor)
      2. Alarm I/O Input 1ea / Output 2ea
      3. Remote Control RS-485
      4. RS-485 Protocol Pelco D/P, Samsung T, Honeywell, Bosch, Panasonic, Sungin,

AD, Vicon and GE

* + - 1. Alarm Triggers Alarm Input, Motion Detection, Video & Audio Analytics,

Network Disconnection

* + - 1. Alarm Events File Upload via FTP and E-mail, Notification via E-mail,

Local storage (SD/SDHC/SDXC) or NAS recording,

External output

* + - 1. Intelligent Analytics Tampering, Loitering, Directional Detection, Virtual Line,

Enter/Exit, Appear/Disappear, Fence Detection

Shock Detection, Motion Detection, Audio Detection,

Temperature Detection

Sound Classification

(Scream / Gunshot / Explosion / Crashing glass)

* + - 1. Pixel Counter Support
      2. Storage Micro SD/SDHC/SDXC 256GB (256GB x 1 slot) , NAS support
    1. Video Streams
       1. Video compression H.265, H.264, MJPEG
       2. Resolution 640x480, 640x360, 320x240
       3. Maximum Framerate
          1. H.265 / H.264 / MJPEG Max. 30fps at all resolutions
       4. WiseStream Ⅱ Support
       5. Bitrate Control Method VBR (H.265 / H.264 / MJPEG), CBR (H.265 /H.264)
       6. Streaming Capability Up to 10 profiles
       7. Streaming Method Unicast / Multicast
       8. Simultaneous Users 20 maximum (Unicast)
       9. Profile set Max. 10 ea
       10. Interoperability ONVIF Profile S / G support, SUNAPI, Open Platform
    2. Audio
       1. Audio In Built in Mic / Line-in / External Mic(2.5VDC/4mA supply)

(Input impedance: approx. 2K Ohm)

* + - 1. Audio Out Line out (3.5mm stereo mini jack)
      2. Audio Compression G.711 u-law / G.726 / AAC Selectable,

G.726 (ADPCM) 8KHz, G.711 8KHz,

G.726: 16 / 24 / 32 / 40Kbps,

AAC-LC: 48Kbps at 8 / 16 / 32 / 48KHz

* + - 1. Communication Bi-directional (2-Way)
    1. Network
       1. Connectivity – 10/100 Base-T Ethernet via RJ-45 connector
       2. Protocol
          1. IP v4 / v6, TCP, UDP
          2. Configuration: DHCP, LLDP
          3. Web service: HTTP, HTTPS
          4. Network Service: ARP, Bonjour, DNS, ICMP, NTP, PIM-SM, SNMP v1/2c/3 – MIB-2, UPnP
          5. Media: RTP, RTCP, RTSP
          6. Multicast: IGMP
          7. Notifications: FTP, SMTP
          8. Remote Access: PPPoE
       3. DDNS – The camera shall support DDNS services offered by the manufacturer and others publicly available service offerings
       4. QoS – Layer 3 DSCP
       5. Security Feature
          1. User password protection
          2. The device shall not provide a manufacture default password. Default password change shall be required to access the camera.
          3. A minimal level of password complexity shall be required by the camera.
          4. The camera shall not have a manufacture back-door password.
          5. The manufacturer shall provide a tool that provides the ability to make password changes to multiple cameras at the same time.
          6. IP address filtering – List of allowed or blocked IP addresses
          7. HTTPS(SSL) login authentication
          8. HTTPS(SSL) secured communication
          9. Digest login authentication
          10. User access log
          11. 802.1x authentication
       6. Discovery – The manufacturer shall offer a discovery program to identify all devices of them on the network.
       7. Configuration – The manufacturer shall offer a configuration program that remotely allows users to change settings on multiple cameras simultaneously.
       8. Firmware upgrade – The manufacturer shall offer a program capable of upgrading multiple cameras at the same time (not requiring access to individual cameras).
       9. Camera backup setting – The manufacturer shall provide a program that provides the ability to save multiple camera settings to a file and restore these camera settings if needed.
       10. Reporting – The manufacturer shall provide a tool that can generate a report including thumbnail view, MAC address, IP address, serial number and other camera settings.
    2. Electrical
       1. Power
          1. Input Voltage / Current PoE (IEEE 802.3af), DC 12V, AC 24V
          2. Power Consumption Max 10W (PoE), Max 9W (DC 12V), Max 10.5W (AC 24V)

Typ. 8.6W (PoE), Typ. 7.5W (DC 12V), Typ. 8.9W (AC 24V)

* + 1. Mechanical and Environmental
       1. Color / Material White(RAL-9003) / Aluminum
       2. Dimensions (W x H x D) *Φ*101.97 x 309mm (*Φ* 4.01" x 12.16")
       3. Weight 2,452g (5.4 lb)
       4. Temperature
          1. Operating -40°C ~ +60°C(-40°F ~ +140°F)
          2. Storage -50°C ~ +60°C (-58°F ~ +140°F)
       5. Humidity Less than 90% RH
       6. Ingression Protection IP66, NEMA 4X
       7. Vandal Resistance IK10

END OF SECTION

1. **EXECUTION**
   1. **INSTALLERS**
      1. Contractor personnel shall comply with all applicable state and local licensing requirements.
   2. **PREPARATION**
      1. The network design and configuration shall be verified for compatibility and performance with the camera(s).
      2. Network configuration shall be tested and qualified by the Contractor prior to camera installation.
      3. All firmware found in products shall be the latest and most up-to-date provided by the manufacturer, or of a version as specified by the provider of the Video Management Application (VMA) or Network Video Recorder (NVR).
      4. All equipment requiring users to log on using a password shall be configured with user/site-specific password/passwords. No system/product default passwords shall be allowed.
   3. **INSTALLATION**
      1. The Contractor shall carefully follow instructions in documentation provided by the manufacturer to insure all steps have been taken to provide a reliable, easy-to-operate system.
      2. All equipment shall be tested and configured in accordance with instructions provided by the manufacturer prior to installation.
      3. Before permanent installation of the system, the Contractor shall test the system in conditions simulating the final installed environment.
   4. **STORAGE**
      1. The hardware shall be stored in an environment where temperature and humidity are in the range specified by the Manufacturer.

END OF SECTION